{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":159,"n_cols":10,"rows_kept":159,"merged":[[0,0,0,9],[2,0,29,0],[2,1,6,1],[7,1,9,1],[10,1,12,1],[13,1,17,1],[18,1,19,1],[21,1,25,1],[26,1,29,1],[30,0,33,0],[30,1,32,1],[34,0,42,0],[34,1,42,1],[43,0,47,0],[43,1,46,1],[48,0,49,0],[48,1,49,1],[50,0,54,0],[50,1,53,1],[55,0,60,0],[55,1,56,1],[57,1,60,1],[57,10,60,10],[61,0,65,0],[61,1,65,1],[66,0,67,0],[66,1,67,1],[68,0,96,0],[68,1,69,1],[70,1,81,1],[83,1,89,1],[90,1,92,1],[93,1,96,1],[97,0,155,0],[97,1,106,1],[97,9,106,9],[107,1,123,1],[124,1,125,1],[126,1,132,1],[133,1,145,1],[146,1,149,1],[150,1,155,1],[157,0,158,0]],"flags":["formulas_cached_only"]}
["试验设备明细单                        附件一"]
["检验项目","参数","序号","仪器名称","规格型号","单位","数量","单价","合计价","备注"]
["混凝土外加剂","PH值",1,"酸度计","PHS-3C","台",1]
[null,null,2,"甘汞电极",null,"个",1]
[null,null,3,"玻璃电极",null,"个",1]
[null,null,4,"复合电极",null,"个",1]
[null,null,5,"分析天平","FA2004","台",1,null,null,"万分之一"]
[null,"密度",1,"比重瓶","25mL或50mL","个",1]
[null,null,2,"干燥器","Ф240","个",1,null,null,"含干燥剂1瓶"]
[null,null,3,"恒温恒湿养护箱","HWHS-II","台",1,null,null,"温度（20±2）℃；相对湿度（60±5）%\n\n砂浆：温度（20±5）℃ 相对湿度（45～ 75）%"]
[null,"细度",1,"电子天平","200g/0.001g","台",1]
[null,null,2,"试验筛","Ф150*50mm/0.315mm","个",1,null,null,"带盖，铜丝网筛布"]
[null,null,3,"试验筛","1.18mm","个",5]
[null,"凝结时间差",1,"混凝土贯入阻力仪","HG-1000","台",1,null,null,"数显式"]
[null,null,2,"圆孔筛","5mm","个",1]
[null,null,3,"吸液管","5mL","个",1]
[null,null,4,"烧杯","300mL","个",1]
[null,null,5,"抹刀",null,"把",1]
[null,"含气量",1,"电子秤","60kg/2g","台",1]
[null,null,2,"混凝土含气量测定仪","CA-3","台",1]
[null,"固体含量（或含水率）",1,"带盖称量瓶","65*25mm","个",1]
[null,"限制膨胀率",1,"限制膨胀率测定仪","BC-158","台",1,null,null,"配千分表,同时做1组（3个）试验。"]
[null,null,2,"纵向限制器",null,"个",9,null,null,"1组3个"]
[null,null,3,"电子天平","2kg/0.01g","台",1]
[null,null,4,"水泥恒温恒湿标准养护箱  ","YH-40B","台",1]
[null,null,5,"恒温水浴","CF-B","台",1]
[null,"泌水率比",1,"混凝土泌水率筒","5L","个",1,null,null,"带盖"]
[null,null,2,"量筒（带塞）","100mL/1mL","个",1]
[null,null,3,"吸液管","5mL","个",1]
[null,null,4,"秒表","0-3600s","个",1,null,null,"0.1s"]
["建筑防水涂料","固体含量",1,"电子天平","200g/0.001g","台",1]
[null,null,2,"干燥器","Ф240","个",1,null,null,"含干燥剂1瓶"]
[null,null,3,"培养皿","Ф60-Ф75mm","个",1]
[null,"耐热性",1,"铝板","120*50*2～3mm","块",1,null,null,"中间上部有小孔"]
["建筑防水卷材","可溶物含量",1,"索氏萃取器","500mL","套",1]
[null,null,2,"试验筛","0.315mm","个",1]
[null,null,3,"滤纸","≧Ф150mm","盒",1]
[null,null,4,"浅盘",null,"个",1]
[null,null,5,"裁刀（防水卷材试件制备模板）",null,"套",1,null,null,"正方形试样"]
[null,null,6,"白色记号笔",null,"支",10]
[null,null,7,"恒温恒湿养护箱","HW-II","台",1,null,null,"防水卷材试件：\n温度(23土2)℃，相对湿度(30～70)%；\n\n防水涂料试件：\n温度(23土2)℃，相对湿度(50土10)%。"]
[null,null,8,"防烫隔热手套",null,"付",5]
[null,null,9,"防毒面罩   ",null,"个",5]
["弹性体改性防水卷材","热老化后低温柔度",1,"电子天平","10kg/0.1g","台",1]
[null,null,2,"数显式游标卡尺","0-300mm","把",1,null,null,"数显式，金属壳。"]
[null,null,3,"滑石粉",null,"袋",1]
[null,null,4,"玻璃板",null,"块",5]
[null,"搭接缝不透水性",1,"电动防水卷材搭接缝不透水仪",null,"台",1]
["建筑防水卷材","接缝剥离强度",1,"防水卷材剥离强度试验附具",null,"套",1,null,null,"用WDW-5微机控制电子万能试验机即可"]
[null,null,2,"防水材料专用附具",null,"套",1,null,null,"更有效用于SBS防水卷材试验，即弹性体改性沥青防水卷材试验，可避免滑脱、撕裂试样"]
["陶瓷砖","吸水率",1,"干燥器  ","Ф240","个",1,null,null,"含干燥剂1瓶"]
[null,null,2,"加热装置",null,"台",1,null,null,"用惰性材料制成的用于煮沸的加热装置；\n将砖竖直地放在盛有去离子水的加热装置中,使砖互不接触，砖的上部和下部应保持有5cm深度的水，煮沸2h。"]
[null,null,3,"电子天平","5kg/0.01g","台",1,null,null,"精度为所测试样质量0.01%"]
[null,null,4,"麂皮（鹿皮）",null,"块",6]
[null,"弯曲强度",1,"陶瓷砖断裂模数和破坏强度测定仪","10000N","台",1,null,null,"试样范围：100×100-1000×1000mm，电动加载，可按国标恒速加载。"]
["天然石材","吸水率",1,"电子天平","1kg/0.01g","台",1]
[null,null,2,"恒温水浴","HW-IIT","台",1,null,null,"底面平整，且带有玻璃棒作为试样支撑，试样边长50mm的正方体或直径、高度均为50 mm的圆柱体，每组五块。\n试样间隔应不小于15mm，加人去离子或蒸馏水(20℃±2℃)，最终水面应超过试样高度25士5mm。\n\n"]
[null,"弯曲强度",1,"石材弯曲附具",null,"套",1]
[null,null,2,"数显游标卡尺","0-300mm","把",1,null,null,"数显式，金属壳。"]
[null,null,3,"万能角度尺","0～320°","把",1,null,null,"不锈钢"]
[null,null,4,"干燥器","Ф240","个",1,null,null,"含干燥剂1瓶"]
["建筑砂浆基本性能","拉伸粘结强度",1,"砂浆拉伸附具",null,"套",1,null,null,"在WDW-5微机控制电子万能试验机上进行试验"]
[null,null,2,"成型框","40*40*6mm","个",10,null,null,"10个1组"]
[null,null,3,"拉拔块","40*40*10mm","个",10,null,null,"10个1组"]
[null,null,4,"钢制垫板","43*43*3mm","个",2]
[null,null,5,"砂浆拉伸粘结强度试模","70*70*20mm","联",3,null,null,"1联3格"]
["混凝土瓦","抗折强度",1,"混凝土瓦抗折附具",null,"套",1,null,null,"在30吨万能试验机上进行试验，出厂标定有效测量范围从5kN开始，衔接WDW-5微机控制电子万能试验机"]
[null,null,2,"钢直尺","0-500mm/1mm","把",1]
["混凝土掺合料","细度",1,"方孔筛","0.045mm","个",5]
[null,null,2,"标准粉（粉煤灰）",null,"瓶",2]
[null,"烧失量",1,"瓷坩埚","30mL","个",5,null,null,"带盖"]
[null,null,2,"坩埚钳",null,"把",1]
[null,null,3,"箱式电阻炉","1200℃","台",1]
[null,null,4,"干燥器","Ф240","个",1,null,null,"含干燥剂1瓶"]
[null,null,5,"烧杯","200mL","个",1]
[null,null,6,"烧杯","400mL","个",1]
[null,null,7,"平头玻璃棒",null,"根",1]
[null,null,8,"中速定量滤纸",null,"盒",1]
[null,null,9,"慢速定量滤纸",null,"盒",1]
[null,null,10,"表面皿","9cm","个",1]
[null,null,11,"胶头擦棒",null,"个",1]
[null,null,12,"快速定量滤纸",null,"盒",1]
[null,"需水量比",1,"电子天平","1kg/0.01g","台",1]
[null,"比表面积",1,"自动比表面积测定仪  ","FBT-9A","台",1]
[null,null,2,"电子天平","200g/0.001g","台",1]
[null,null,3,"秒表","0-3600s","个",1,null,null,"0.1s"]
[null,null,4,"方孔筛","0.9mm","个",5]
[null,null,5,"毛刷",null,"把",1]
[null,null,6,"小匙",null,"把",1]
[null,null,7,"基准材料（水泥比表面积标准粉）",null,"瓶",1]
[null,"活性指数",1,"电子天平","2kg/0.01g","台",1]
[null,null,2,"水泥胶砂量水器","225mL","个",1]
[null,null,3,"橡皮锤",null,"把",1]
[null,"流动度比",1,"小刀",null,"把",1,null,null,"刀口平直，长度大于80mm"]
[null,null,2,"数显游标卡尺","0-300mm","把",1,null,null,"数显式，金属壳。"]
[null,null,3,"浅盘",null,"个",1]
[null,null,4,"料铲",null,"把",1]
["化学","水泥氯离子含量GB/T176-2017（6.13）",1,"分析天平","FA2004","台",1,null,null,"硫氰酸铵容量法（基准法）"]
[null,null,2,"烧杯","400mL","个",1]
[null,null,3,"量筒","50mL","个",1]
[null,null,4,"玻璃棒",null,"根",1]
[null,null,5,"电炉",null,"个",1]
[null,null,6,"移液管","5mL","个",1]
[null,null,7,"玻璃砂芯漏斗",null,"个",1]
[null,null,8,"抽吸装置",null,"套",1]
[null,null,9,"锥形瓶","250mL","个",1]
[null,null,10,"温度计",null,"个",1]
[null,"亚甲蓝值与石粉含量",1,"电子天平","1kg/0.01g","台",1]
[null,null,2,"方孔筛","0.08mm","个",1]
[null,null,3,"方孔筛","1.25mm","个",1]
[null,null,4,"容器",null,"个",1,null,null,"深度大于 250mm"]
[null,null,5,"移液管","2mL","个",1]
[null,null,6,"移液管","5mL","个",1]
[null,null,7,"亚甲蓝试验装置",null,"台",1]
[null,null,8,"秒表","0-3600s","个",1,null,null,"0.1s"]
[null,null,9,"容量瓶","1000mL","个",1]
[null,null,10,"温度计","0-250℃/1℃","个",1]
[null,null,11,"玻璃棒","Ф8*300mm","根",1]
[null,null,12,"搪瓷盘",null,"个",1]
[null,null,13,"毛刷",null,"把",1]
[null,null,14,"烧杯","100mL","个",1]
[null,null,15,"烧杯","500mL","个",1]
[null,null,16,"烧杯","1000mL","个",1]
[null,null,17,"电炉","0-2000W","台",1]
[null,"压碎指标",1,"瓷盘",null,"个",10]
[null,null,2,"小勺",null,"把",2]
[null,"砂中氯离子含量\nJGJ/52-2006（6.18）",1,"电子天平","2kg/0.01g","台",1]
[null,null,2,"带塞磨口瓶","1000mL","个",1]
[null,null,3,"三角瓶","300mL","个",1]
[null,null,4,"滴定管","10mL或25mL","个",1]
[null,null,5,"容量瓶","500mL","个",1]
[null,null,6,"移液管","2mL","个",1]
[null,null,7,"移液管","50mL","个",1]
[null,"混凝土氯离子含量\nGB/T11896-1989\n(1-8)",1,"吸管","25mL","个",1]
[null,null,2,"吸管","50mL","个",1]
[null,null,3,"锥形瓶","250mL","个",2]
[null,null,4,"棕色滴定管","25mL","个",1]
[null,null,5,"瓷坩埚",null,"个",1]
[null,null,6,"干燥器","Ф240","个",1,null,null,"含干燥剂1瓶"]
[null,null,7,"分析天平（万分之一）","FA2004","台",1]
[null,null,8,"容量瓶","1000mL","个",1]
[null,null,9,"棕色瓶","1000mL","个",1]
[null,null,10,"玻璃棒",null,"根",1]
[null,null,11,"瓷蒸发皿",null,"个",1]
[null,null,12,"箱式电阻炉","1200℃","台",1]
[null,null,13,"恒温水浴",null,"台",1]
[null,"拌合用水氯离子含量\nJGJ/T 322-2013\n(附录A)",1,"氯离子选择电极",null,"瓶",1]
[null,null,2,"参比电极",null,"个",1,null,null,"应为双盐桥饱和甘汞电极"]
[null,null,3,"电位测量仪器",null,"台",1]
[null,null,4,"快速定量滤纸",null,"盒",1]
[null,"混凝土外加剂氯离子含量\nGB/T8077-2023",1,"全自动氯离子含量测定仪",null,"台",1]
[null,null,2,"移液管","10mL","个",1]
[null,null,3,"分析天平（万分之一）","FA2004","台",1]
[null,null,4,"称量瓶",null,"个",1]
[null,null,5,"干燥器","Ф240","个",1,null,null,"含干燥剂1瓶"]
[null,null,6,"表面皿","9cm","个",1]
["砖回弹法",null,1,"砖回弹仪","HT75-A","台",2]
["干燥箱",null,1,"电热鼓风干燥箱","101-2A","台",1]
[null,null,2,"电热鼓风干燥箱","101-3B","台",1]